|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | Beneteau 321First - 2000719 Ed |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135,150 etc.)" | Luff Leech and foot | HEL P |
| H2 | Luff Length, Max Hoist, B measurement | 39.40 FEET webbing loop tip to webbing loop tip (Max)(38.80ft Net Finished size day of delivery) | HEL P |
| H3 | Leech Length | 38.50 FEET | HEL P |
| H4 | Foot Length | 19.6 FEET | HEL P |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0- Ring) | PRESSED RING | HEL P |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | N/A | HEL P |
| H11 | Track 2 (Tack to Genoa Track Ending) | N/A | HEL P |
| H12 | Vessel "I" Measurement | 42.08 FEET | HEL P |
| H13 | Vessel "J" Measurement | 12.25 FEET | HEL P |

|  |  |  |  |
| --- | --- | --- | --- |
| H14 | Calculated Forestay Length | N/A |  |
| H15 | Reef | N/A |  |
| H16 | LP | N/A | HEL P |
| H17 | Color of Suncover | Blue | HEL P |
| H18 | Side of Sail for Suncover (port or Stbd) | Stbd |  |
| H19 | Luff Tape Size (such as #6) | 1/4 INCH | HEL P |
| H20 | Furler Manufacturer | Factor SD 130 |  |
| H21 | Foam Luff | Yes | HEL P |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | HEL P |
| H25 | Telltail Window | YES |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | HEL P |
| H28 | Cloth Weight | 7.88 |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | HEL P |

|  |  |  |  |
| --- | --- | --- | --- |
| H30 | Sheeting Stripe (red, blue, black) | No | HEL P |
| H31 | Draft Stripe Color (red, blue or black) | NO | HEL P |
| H32 | Clew Height off Deck | sailmaker | HEL P |
| H33 | Tack Height off Deck | 17 INCHES | HEL P |
| H34 | Luff tape starts 21in up from Tack | 21 INCHES | HEL P |
| H35 | Specialty Sail | No | HEL P |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | HEL P |