|  |  |  |  |
| --- | --- | --- | --- |
|  | - Mainsail - | 3000106 Frederic |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 5.5 inches (“A” dimension) | [HELP](http://www.fareastsails.com/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 1.75 inches (“B” dimension)  “C” dimension is 17.25” | [HELP](http://www.fareastsails.com/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | N/A | [HELP](http://www.fareastsails.com/orderimages/Clew%20X%20and%20Y.jpg) |
| M4 | Clew type (slug, outhaul car or ring with strap) | Webbing  to slug (no stainless steel) (A032, 9.3mm by 3.0mm by 50mm) | [HELP](http://www.fareastsails.com/orderimages/Clew_Types_Fareastsails.html) |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.com/orderimages/weathermax_colors.html) |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.com/orderimages/Boom_offsets.html) |
| M7 | Headboard | Please use short diagonal batten in lieu of headboard (see sailplan for head dimensions) | [HELP](http://www.fareastsails.com/orderimages/Head_Board_Types.jpg) |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | webbing only | [HELP](http://www.fareastsails.com/orderimages/Tack_Ring_Type.html) |
| M11 | Tack angle | Please see sailplan provided for leach measurement which will dictate the angle. (head to clew is 35.7 feet | [HELP](http://www.fareastsails.com/orderimages/Tack_Angle.html) |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.com/orderimages/Jack_Line.jpg) |
| M13 | Mast Bend (Luff Round) | Please see http://antrim27.org/tuning.html , triple spreader CST carbon mast for luff curve details  5mm | [HELP](http://www.fareastsails.com/orderimages/mastbend.jpg) |
| M14 | Fractional Rig (Yes, No) | Yes | [HELP](http://www.fareastsails.com/orderimages/Fractional%20Rig.jpg) |
| M15 | Mast - Keel or Deck Stepped? | Deck Stepped |  |
| M16 | Number of Reefs | 2  Reefs | [HELP](http://www.fareastsails.com/orderimages/Reefs.html) |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | N/A | [HELP](http://www.fareastsails.com/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.com/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M19 | Reefing Ring Type | Webbing only; no stainless steel please | [HELP](http://www.fareastsails.com/orderimages/Reefing_Ring_Types.html) |
| M20 | Luff Length (Max Hoist - P) | Please see sailplan “Antrim 27 Class Mainsail” P is shown as 33.75 feet Max  (Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.com/orderimages/Mainsail%20Luff%20Measurement.html) |
| M21 | Foot Length (Max Foot - E) | See attachment, E is 14.0 feet Max  (Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Foot_Measurement.html) |
| M22 | Leech Length (straight line head to clew) | Sailmaker See attachment, head to clew measurement is 35.7 feet | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Leech_Measurement_Check.html) |
| M23 | Bimini to Clear (yes or no) | No | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | The Antrim 27 has no backstay | [HELP](http://www.fareastsails.com/orderimages/BoomArt2.jpg) |
| M27 | Luff Slides (Part Number) | Bolt Rope HR6 | [HELP](http://www.fareastsails.com/orderimages/sailslides3.html) |
| M28 | Foot Slides (Part Number) | None, loose footed  except at Clew (A032, 9.3mm by 3.0mm by 50mm) | [HELP](http://www.fareastsails.com/orderimages/sailslides3.html) |
| M29 | Roach Type | See sail plan | [HELP](http://www.fareastsails.com/orderimages/roach.jpg) |
| M30 | Roach Factor | See Sail Plan | [HELP](http://www.fareastsails.com/Roach-Factor.html) |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Design%20MGM%20and%20MGU.html) |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Design%20MGM%20and%20MGU.html) |
| M33 | Batten Type (Partial or Full) | 4 full  1 Partial   See sail Plan as for girth dimensions at batten tips  Our battens are as follows:   * + Top 4’ 8.25”   + #2 7’ 9.125”   + #3 10’ 1.25”   + #4  12’ 1.375”   + #5  6’ 5.25” | [HELP](http://www.fareastsails.com/orderimages/Full%20Batten%20Options.html) |
| M34 | Include Battens | N/A |  |
| M35 | Install Nylon Batten Holders | YES | [HELP](http://www.fareastsails.com/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html) |
| M36 | Intermediate Sliders | YES | [HELP](http://www.fareastsails.com/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html) |
| M37 | Cloth Weight | 6.11 Warp Drive |  |
| M38 | Cut Type | Tri Radial |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | Yes, please use webbing, no stainless | [HELP](http://www.fareastsails.com/orderimages/cunningham.jpg) |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.com/orderimages/telltails.html) |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | Yes, Red | [HELP](http://www.fareastsails.com/orderimages/snlogos.html) |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | Yes, Red, USA 6 | [HELP](http://www.fareastsails.com/orderimages/snlogos.html) |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Color?) Red | [HELP](http://www.fareastsails.com/Draft%20Stripe.html) |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.com/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.com/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.com/orderimages/Lazy_Bag.html) |