Main comments

-increase roach: 1/2 luff width 10ft, ¾ luff width 6ft 1/4in– I measured these on my current sail - distance measured from leach to slip rope forward side.

-add 1 more partial batten

-reduce foot to 15.5ft

-increase luff to 45.2ft

-change slides to A014 Seldon (I found a reference)

-head slide A114 Seldon allslip (I found a reference)

-add spreader patches – see below drawing below for center locations.

-change to 3 draft stripes

-move reef point to 5ft 10in from foot

