|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Mainsail -  | 3000409 Brian |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 46mm | [HELP](http://www.fareastsails.com/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
|  |  |  |  |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 30mm | [HELP](http://www.fareastsails.com/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | 45mm | [HELP](http://www.fareastsails.com/orderimages/Clew%20X%20and%20Y.jpg)  |
| M4 | Clew type (slug, outhaul car or ring with strap) | Press ring with slug – A033 | [HELP](http://www.fareastsails.com/orderimages/Clew_Types_Fareastsails.html)  |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.com/orderimages/weathermax_colors.html)  |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.com/orderimages/Boom_offsets.html)  |
| M7 | Headboard | Yes | [HELP](http://www.fareastsails.com/orderimages/Head_Board_Types.jpg)  |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | #2 tack press ring  | [HELP](http://www.fareastsails.com/orderimages/Tack_Ring_Type.html)  |
| M11 | Tack angle | 88.5 | [HELP](http://www.fareastsails.com/orderimages/Tack_Angle.html)  |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.com/orderimages/Jack_Line.jpg)  |
| M13 | Mast Bend (Luff Round) | Std | [HELP](http://www.fareastsails.com/orderimages/mastbend.jpg)  |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.com/orderimages/Fractional%20Rig.jpg)  |
| M15 | Mast - Keel or Deck Stepped? | Deck Stepped |  |
| M16 | Number of Reefs | 2  Reefs | [HELP](http://www.fareastsails.com/orderimages/Reefs.html)  |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | yes | [HELP](http://www.fareastsails.com/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.com/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M19 | Reefing Ring Type | Grommet through sail | [HELP](http://www.fareastsails.com/orderimages/Reefing_Ring_Types.html)  |
| M20 | Luff Length (Max Hoist - P) | 35ft  Max(34.47ft Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.com/orderimages/Mainsail%20Luff%20Measurement.html)  |
| M21 | Foot Length (Max Foot - E) | 12ft  Max(11.32m Net Finished size day of Delivery)  | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Foot_Measurement.html)  |
| M22  | Leech Length (straight line head to clew) | Sailmaker | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Leech_Measurement_Check.html)  |
| M23 | Bimini to Clear (yes or no) | N/A | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | 15' 5" | [HELP](http://www.fareastsails.com/orderimages/BoomArt2.jpg)  |
| M27 | Luff Slides (Part Number) | A009 with shackles | [HELP](http://www.fareastsails.com/orderimages/sailslides3.html)  |
| M28 | Foot Slides (Part Number) | HR6 bolt rope | [HELP](http://www.fareastsails.com/orderimages/sailslides3.html)  |
| M29 | Roach Type | Cruise | [HELP](http://www.fareastsails.com/orderimages/roach.jpg)  |
| M30 | Roach Factor | 1.07 | [HELP](http://www.fareastsails.com/Roach-Factor.html)  |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Design%20MGM%20and%20MGU.html)  |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Design%20MGM%20and%20MGU.html)  |
| M33 | Batten Type (Partial or Full) | 4 Partial | [HELP](http://www.fareastsails.com/orderimages/Full%20Batten%20Options.html)  |
| M34 | Include Battens | Yes |  |
| M35 | Install Nylon Batten Holders | N/A | [HELP](http://www.fareastsails.com/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html)  |
| M36 | Intermediate Sliders | N/A | [HELP](http://www.fareastsails.com/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html)  |
| M37 | Cloth Weight | 7.88 |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | No | [HELP](http://www.fareastsails.com/orderimages/cunningham.jpg)  |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.com/orderimages/telltails.html)  |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](http://www.fareastsails.com/orderimages/snlogos.html)  |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | No | [HELP](http://www.fareastsails.com/orderimages/snlogos.html)  |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Black) | [HELP](http://www.fareastsails.com/Draft%20Stripe.html)  |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.com/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.com/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.com/orderimages/Lazy_Bag.html) |

M1 picture

 

M1 jaw width 1 inch or 25.4mm

M2 picture

 measured straight across boom, made a mark

 measured up

M3 picture

 X measurement

 Y measurement

M4 pictures







M19 pictures



M27 pictures





