|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Headsail - | 3001102 Henrik |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | Luff Leech and Foot | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fgen123.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363475161&sdata=tbbomxON2hCw14xjYKe5Ec3YUEH0zS8tCOywbYXBptk%3D&reserved=0)  |
| H2 | Luff Length, Max Hoist, B measurement | 16.81m webbing loop tip to webbing loop tip (Max)(16.55m Net Finished size day of delivery) | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FFurler_Luff_Measurement.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363485172&sdata=cDLEnfVNUa5BcdKG%2BX85PRcmeTcj%2FsJ1AtpD0W5m5MI%3D&reserved=0)  |
| H3 | Leech Length | 16.05m | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FLeech%2520Length.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363495178&sdata=O8y8EmE85xvY2TvzJ2w%2BY0ivzrInmPTsQX9lxUwqB8M%3D&reserved=0)  |
| H4 | Foot Length | 7.37m | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FFoot%2520Length.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363505189&sdata=N%2BJoPD3MVzp8wtadg0HZFcgpOWJzPJNiLfLkm7Qk6fk%3D&reserved=0)  |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press ring | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fgenoa%2520clew%2520types.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363515194&sdata=8hKWS85mQhCGFnmdZC41VNUiRr3t2ZY8Uh9XK3R0ez4%3D&reserved=0)  |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | N/A | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FGenoa%2520Track.pdf&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363515194&sdata=p4Dj2vhRrmmYZKcfmYgGoh4R6i41WuzzEsdBQ0PYBWk%3D&reserved=0)  |
| H11 | Track 2 (Tack to Genoa Track Ending) | N/A | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FGenoa%2520Track.pdf&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363525206&sdata=yWnZBZHkKJkw5lAZFbmKmiU9IX9X%2B5JiC8AtvDcF9o8%3D&reserved=0)  |
| H12 | Vessel "I" Measurement | N/A  | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FVessel%2520I%2520measurement.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363535211&sdata=YSPWowvfIvi7iXXgAjh%2B%2Fq2asgilOd5eSHk5n7yGvB8%3D&reserved=0)  |
| H13 | Vessel "J" Measurement | N/A  | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FLP%2BI%2BJ.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363545222&sdata=x8fAFNooP%2F9873t5q7wN4Xi8HAMVQwMLs1dpswivlLY%3D&reserved=0)  |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sailmaker | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FLP.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363555233&sdata=A2%2FIgCYoE%2BfJxCFwJRST%2BGBBpNw6mcQbNAqcpJd48tQ%3D&reserved=0)  |
| H17 | Color of Suncover | Pacific Blue | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fweathermax_colors.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363565233&sdata=zyt3k6GMZaz576ULPeVlGQIbuZT9%2F%2BL7pUJQgkoW64s%3D&reserved=0)  |
| H18 | Side of Sail for Suncover (port or Stbd) | port |  |
| H19 | Luff Tape Size (such as #6) | 6mm Finished Size | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FFurler_Luff_Tape.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363575244&sdata=yzWJQRcE2fpMq6m6h5ems3wbmmozuuTmru5ERjaqseg%3D&reserved=0)  |
| H20 | Furler Manufacturer | N/A |  |
| H21 | Foam Luff | Yes | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FFoam_Luff.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363585249&sdata=Gkiw3hZFyd5s4Ne4v0YG8V2wTPxh6NjDsY95AzAhqgQ%3D&reserved=0)  |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Ftelltails.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363595261&sdata=qsQ2FQASn0dy6L3eMdnFp2EoWj72TBWp7FJoI8Xw0Qs%3D&reserved=0)  |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fsnlogos.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363605278&sdata=CBxjIYZCkMvkzcKoolsikxLlxNYoIxFlkuK6GM3hXMU%3D&reserved=0) |
| H28 | Cloth Weight | 10.88 |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fsnlogos.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363615283&sdata=Zlyagm2PpN8JgrG%2FZEovfeYntFlTu2YMjvd6qWvpP4I%3D&reserved=0)  |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FSheeting%2520Stripe.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363625282&sdata=TVXBy0w%2BLrey%2FrQXQ7%2FtKgvaELRMtuzvbLUDvpEjNCk%3D&reserved=0)  |
| H31 | Draft Stripe Color  (red, blue or black) | Yes Blue | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FDraft%2520Stripe.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363635300&sdata=2yx27K38vAB3CQQORS%2Bv%2BBschGA7qAhylt6QPS4vdD0%3D&reserved=0)  |
| H32 | Clew Height off Deck | sailmaker | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fclewheight.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363645299&sdata=oTopq3V0oFdaqNeav2uemEnqWrbfj88iuHozplS4LKc%3D&reserved=0)  |
| H33 | Tack Height off Deck | 46 cm | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2Fclewheight.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363655310&sdata=EfrYkkaaBLWkX2ulsXtvxTL80VQ%2BDTOdItN2DkDRAZg%3D&reserved=0)  |
| H34 | Luff tape starts 100cm up from Tack | 100 cm | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FLuff%2520tape%2520start.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363665322&sdata=Mcl7PeJFGGNkyyipJ2%2BcvR3UzfSP2TXOE0sYYCdwFTM%3D&reserved=0) |
| H35 | Specialty Sail | No | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FSpecialty%2520Sails.html&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363675321&sdata=nzCgM0jElkoTba%2BPkBRCha9AsqPZ2lLuP4l7UrW3Zh4%3D&reserved=0) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](https://apc01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.fareastsails.info%2Forderimages%2FLP.jpg&data=02%7C01%7C%7Cd030820341074388471308d772b7ded6%7C84df9e7fe9f640afb435aaaaaaaaaaaa%7C1%7C0%7C637104006363685338&sdata=7nXVehQMmgEyMXo3eRl5cOQepzrNLa0i1spgFJbZN3Y%3D&reserved=0) |