|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | 3001114 David |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | Luff Leech and Foot | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 36’ 7” webbing loop tip to webbing loop tip (Max)  (36.03ft Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | 33’9” | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg) |
| H4 | Foot Length | 16’5” | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg) |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 17’7” | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | 23’7” | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H12 | Vessel "I" Measurement | 35’10” | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| H13 | Vessel "J" Measurement | 11’6” | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | N/A |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | Pacific Blue | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | stbd |  |
| H19 | Luff Tape Size (such as #6) | 5mm | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | Furlex |  |
| H21 | Foam Luff | YES | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 8.88 |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (blue) | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html) |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | N/A | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts 37”up from Tack | 37” | [HELP](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |