|  |  |  |  |
| --- | --- | --- | --- |
|  | - Mainsail - | 4000137 Talo |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 8.5cm | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 4.5cm | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/Clew%20X%20and%20Y.jpg) |
| M4 | Clew type (slug, outhaul car or ring with strap) | D ring with bar | [HELP](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html) |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.info/orderimages/Boom_offsets.html) |
| M7 | Headboard | D ring – see picture  Cut back 6,4 cm | [HELP](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg) |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | D ring with bar | [HELP](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html) |
| M11 | Tack angle | Luff Leech and foot | [HELP](http://www.fareastsails.info/orderimages/Tack_Angle.html) |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.info/orderimages/Jack_Line.jpg) |
| M13 | Mast Bend (Luff Round) | Std | [HELP](http://www.fareastsails.info/orderimages/mastbend.jpg) |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.info/orderimages/Fractional%20Rig.jpg) |
| M15 | Mast - Keel or Deck Stepped? | Keel |  |
| M16 | Number of Reefs | 3 Reefs | [HELP](http://www.fareastsails.info/orderimages/Reefs.html) |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | YES | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M19 | Reefing Ring Type | Press Ring | [HELP](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html) |
| M20 | Luff Length (Max Hoist - P) | 17.90 m Max  (17.63m Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.info/orderimages/Mainsail%20Luff%20Measurement.html) |
| M21 | Foot Length (Max Foot - E) | 5.70 m Max  (5.61m Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Foot_Measurement.html) |
| M22 | Leech Length (straight line head to clew) | Sailmaker | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html) |
| M23 | Bimini to Clear (yes or no) |  | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | ??? | [HELP](http://www.fareastsails.info/orderimages/BoomArt2.jpg) |
| M27 | Luff Slides (Part Number) | Harken  8.4cm cm cut back  Luff box  8,00.cm by 5,00 cm picture. | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html) |
| M28 | Foot Slides (Part Number) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html) |
| M29 | Roach Type | Cruise | [HELP](http://www.fareastsails.info/orderimages/roach.jpg) |
| M30 | Roach Factor | 1.1 | [HELP](http://www.fareastsails.info/orderimages/Roach-Factor.html) |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html) |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html) |
| M33 | Batten Type (Partial or Full) | 1°. 1,36,5 cm.  2°. 2,49    cm  3°  3.41    cm.  4°  4.20    cm.  5°  5.92,5 cm. | [HELP](http://www.fareastsails.info/orderimages/Full%20Batten%20Options.html) |
| M34 | Include Battens | NO |  |
| M35 | Install Nylon Batten Holders | YES | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html) |
| M36 | Intermediate Sliders | YES  1 Webbing Loops  B 5,4 cm. | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html) |
| M37 | Cloth Weight | 10.18 |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sail Maker |  |
| M40 | Cunningham | No | [HELP](http://www.fareastsails.info/orderimages/cunningham.jpg) |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Red) | [HELP](http://www.fareastsails.info/Draft%20Stripe.html) |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | YES – Toast  High, 1,20 cm harken cars.  Around mast 82 cm.  Baton mast connected to the  Boom  around the mast 90 .cm  Long..of the Lazy Bag 5,80 cm.  High of the end of the bag 20cm.  I do have Lazy lines of 4 in each side all adjustable  .pls. | [HELP](http://www.fareastsails.info/orderimages/Lazy_Bag.html) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | 4000137 Talo |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 120 | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 19,75 webbing loop tip to webbing loop tip (Max)  (19.45m Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg) |
| H4 | Foot Length | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg) |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | ??? | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | ??? | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H12 | Vessel "I" Measurement | 18.97m | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| H13 | Vessel "J" Measurement | 5.50m | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | Toast | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | ??? |  |
| H19 | Luff Tape Size (such as #6) | 5mm | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | Harken |  |
| H21 | Foam Luff | YES | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 10.18 |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (Black) | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html) |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | 346mm | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts 248mm up from Tack | 248mm | [HELP](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |