|  |  |  |  |
| --- | --- | --- | --- |
|  | - Mainsail - LAGOON 470 | 4000229 Carlos |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 4.445cm | HELP |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 10cm | HELP |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | We use a sheet for the outhaulLoose Footed | HELP |
| M4 | Clew type (slug, outhaul car or ring with strap) | O Ring With Slug #1 | HELP |
| M5 | Sunbrella clew cover for Furling Mains | na | HELP |
| M6 | Other Offsets |  | HELP |
| M7 | Headboard | Yes | HELP |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | Press Ring on current sail but would consider changing to Webbed | HELP |
| M11 | Tack angle | Mast leans aft approximately 5 degrees. | HELP |
| M12 | Jack Line | No | HELP |
| M13 | Mast Bend (Luff Round) | Std | HELP |
| M14 | Fractional Rig (Yes, No) | No | HELP |
| M15 | Mast - Keel or Deck Stepped? | Deck Stepped |  |
| M16 | Number of Reefs | 2  Reefs + 1 Cunningham | HELP |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | YES | HELP |
| M18 | Foot Reefing Grommets (next to boom) | No | HELP |
| M19 | Reefing Ring Type | Grommet through sail #1 | HELP |
| M20 | Luff Length (Max Hoist - P) | 13.40m(13.26m Net Finished size day of Delivery) | HELP |
| M21 | Foot Length (Max Foot - E) | 6.04m(5.97m Net Finished size day of Delivery) | HELP |
| M22 | Leech Length (straight line head to clew) | 14.25m(14.10m Net Finished size day of Delivery) | HELP |
| M23 | Bimini to Clear (yes or no) | n/a | HELP |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | HELP |
| M26 | Vessel Backstay Measurement | N/A | HELP |
| M27 | Luff Slides (Part Number) | Sail is attached to mast  | HELP |
| M28 | Foot Slides (Part Number) | Loose Footed | HELP |
| M29 | Roach Type | Cruise CAT | HELP |
| M30 | Roach Factor | 1.35 | HELP |
| M31 | MGM | Sailmaker | HELP |
| M32 | MGU | Sailmaker | HELP |
| M33 | Batten Type (Partial or Full) | 6 Full | HELP |
| M34 | Include Battens | No |  |
| M35 | Install Nylon Batten Holders | N/A | HELP |
| M36 | Intermediate Sliders | N/A | HELP |
| M37 | Cloth Weight | 10.88 |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | YES | HELP |
| M41 | Telltails | Yes | HELP |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | HELP |
| M44 | Sail Logo Artwork | YESVessel Name: La BonitaDark Blue |  |
| M45 | Sail Numbers and Color | No | HELP |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Dark Blue) | HELP |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | HELP |
| M49 | Boom Cover | No | HELP |
| M50 | Lazy Bag | No | HELP |