|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Mainsail - | 4000303 Matthew |  |
| M0 | Sail Layout |  |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 5 ½ inch | [HELP](http://www.fareastsails.com/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 2 ½ inch | [HELP](http://www.fareastsails.com/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | See below (M4) | [HELP](http://www.fareastsails.com/orderimages/Clew%20X%20and%20Y.jpg) |
| M4 | Clew type (slug, outhaul car or ring with strap) | Outhaul carY=1/2 inchX=1 inchZ=3/4 inch25mm | [HELP](http://www.fareastsails.com/orderimages/Clew_Types_Fareastsails.html) |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.com/orderimages/weathermax_colors.html) |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.com/orderimages/Boom_offsets.html) |
| M7 | Headboard | Yes | [HELP](http://www.fareastsails.com/orderimages/Head_Board_Types.jpg) |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | 25mm tack pressed ring | [HELP](http://www.fareastsails.com/orderimages/Tack_Ring_Type.html) |
| M11 | Tack angle | 88.5 | [HELP](http://www.fareastsails.com/orderimages/Tack_Angle.html) |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.com/orderimages/Jack_Line.jpg) |
| M13 | Mast Bend (Luff Round) | Std | [HELP](http://www.fareastsails.com/orderimages/mastbend.jpg) |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.com/orderimages/Fractional%20Rig.jpg) |
| M15 | Mast - Keel or Deck Stepped? | Deck |  |
| M16 | Number of Reefs | 2  Reefs | [HELP](http://www.fareastsails.com/orderimages/Reefs.html) |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | Yes | [HELP](http://www.fareastsails.com/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.com/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M19 | Reefing Ring Type | Floppy reefing ring 4 inch | [HELP](http://www.fareastsails.com/orderimages/Reefing_Ring_Types.html) |
| M20 | Luff Length (Max Hoist - P) | 37 feet edge to edge  Max(36.44ft Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.com/orderimages/Mainsail%20Luff%20Measurement.html) |
| M21 | Foot Length (Max Foot - E) |   13 feet 6 inch edge to edge Max(13.29ft Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Foot_Measurement.html) |
| M22 | Leech Length (straight line head to clew) | Sailmaker | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Leech_Measurement_Check.html) |
| M23 | Bimini to Clear (yes or no) | N/A | [HELP](http://www.Fareastsails.com/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | 15 feet 2 inches | [HELP](http://www.fareastsails.com/orderimages/BoomArt2.jpg) |
| M27 | Luff Slides (Part Number) | BO15ss | [HELP](http://www.fareastsails.com/orderimages/sailslides3.html) |
| M28 | Foot Slides (Part Number) | AO18 | [HELP](http://www.fareastsails.com/orderimages/sailslides3.html) |
| M29 | Roach Type | Cruise | [HELP](http://www.fareastsails.com/orderimages/roach.jpg) |
| M30 | Roach Factor | 1.1 | [HELP](http://www.fareastsails.com/Roach-Factor.html) |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Design%20MGM%20and%20MGU.html) |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.com/orderimages/Design%20MGM%20and%20MGU.html) |
| M33 | Batten Type (Partial or Full) | 4 full | [HELP](http://www.fareastsails.com/orderimages/Full%20Batten%20Options.html) |
| M34 | Include Battens | No |  |
| M35 | Install Nylon Batten Holders | YES | [HELP](http://www.fareastsails.com/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html) |
| M36 | Intermediate Sliders | YES2 between each batten | [HELP](http://www.fareastsails.com/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html) |
| M37 | Cloth Weight | 8.88 |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | No | [HELP](http://www.fareastsails.com/orderimages/cunningham.jpg) |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.com/orderimages/telltails.html) |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | Black | [HELP](http://www.fareastsails.com/orderimages/snlogos.html) |
| M44 | Sail Logo Artwork | Black[See Link](http://www.fareastsails.com/orders/2000810Stu/logo.pdf)Searunner trimaran LOGO |  |
| M45 | Sail Numbers and Color | N/A | [HELP](http://www.fareastsails.com/orderimages/snlogos.html) |
| M46 | Draft Stripe and Color(red, blue or black) | Yes Black | [HELP](http://www.fareastsails.com/Draft%20Stripe.html) |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.com/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.com/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.com/orderimages/Lazy_Bag.html) |