|  |  |  |
| --- | --- | --- |
|  |  - Headsail - | 4000812 Andrew |
| H0 | Sail Layout | Not Yet Posted |
| H1 | Size of Headsail (110, 135, 150 etc.)" | Behind the mast furler |
| H2 | Luff Length, Max Hoist, B measurement | 8520mm webbing loop tip to webbing loop tip (Max)(Net Finished size day of delivery) |
| H3 | Leech Length | 8950mm |
| H4 | Foot Length | 3800mm |
| H5 | Tack and Head Fittings | Webbing Loops |
| H6 | Clew Type (Press ring or 0-Ring) | **???** |
| H7 | Leech Line | Yes |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |
| H9 | Foot Line | Yes |
| H10 | Track 1 (Tack to Genoa Track Beginning) | N/A |
| H11 | Track 2 (Tack to Genoa Track Ending) | N/A |
| H12 | Vessel "P" Measurement | **???** |
| H13 | Vessel "E" Measurement | **???**  |
| H14 | Roach | 1.03 |
| H15 | Reef | N/A |
| H16 | LP | Sailmaker |
| H17 | Color of Suncover | **???**  |
| H18 | Side of Sail for Suncover (port or Stbd) | **???**  |
| H19 | Luff Tape Size (such as #6) | **???**  |
| H20 | Furler Manufacturer | **???**  |
| H21 | Foam Luff | N/A |
| H22 | Cut Type | Cross |
| H23 | Sail Area | Sailmaker |
| H24 | Telltails | Yes |
| H25 | Telltail Window | No |
| H26 | Triple Stitch | YES |
| H27 | Logo | No |
| H28 | Cloth Weight | 6.63 |
| H29 | Sail Numbers and Color (red, blue or black) | No |
| H30 | Sheeting Stripe (red, blue, black) | No |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (**color ?**) |
| H32 | Clew Height off Deck | sailmaker |
| H33 | Tack Height off Deck | **???**  |
| H34 | Luff tape starts **???** up from Tack | **???**  |
| H35 | Specialty Sail | No |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  |