|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Headsail - | 5000125 Joel |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 110% | HELP  |
| H2 | Luff Length, Max Hoist, B measurement | 37’4 ½” MAXNet = 37.00ft | HELP  |
| H3 | Leech Length | sailmaker | HELP  |
| H4 | Foot Length | sailmaker | HELP  |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press | HELP  |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) |  | HELP  |
| H11 | Track 2 (Tack to Genoa Track Ending) | ???  | HELP  |
| H12 | Vessel "I" Measurement | 40”4” | HELP  |
| H13 | Vessel "J" Measurement | 13”2’ | HELP  |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sailmaker | HELP  |
| H17 | Color of Suncover | Ocean Blue  | HELP  |
| H18 | Side of Sail for Suncover (port or Stbd) | Starboard  |  |
| H19 | Luff Tape Size (such as #6) | 5.5mm | HELP  |
| H20 | Furler Manufacturer | Schaeffer  |  |
| H21 | Foam Luff | Yes | HELP  |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | HELP  |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | HELP |
| H28 | Cloth Weight | 7.3 HM |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | HELP  |
| H30 | Sheeting Stripe (red, blue, black) | No | HELP  |
| H31 | Draft Stripe Color  (red, blue or black) | Yes Blue | HELP  |
| H32 | Clew Height off Deck | sailmaker | HELP  |
| H33 | Tack Height off Deck | 26”  | HELP  |
| H34 | Luff tape starts 9in up from Tack | 9”  | HELP |
| H35 | Specialty Sail | No | HELP |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | HELP |