|  |  |  |
| --- | --- | --- |
|  | - Mainsail - | 5000226 Claudia |
| M0 | Sail Layout | Not Yet Posted |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 80mm |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 20mm |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | 45mm |
| M4 | Clew type (slug, outhaul car or ring with strap) | Press Ring |
| M5 | Sunbrella clew cover for Furling Mains | na |
| M6 | Other Offsets |  |
| M7 | Headboard | Yes  Headboard to fit  RON-RC26160 |
| M8 | Leech Line | yes |
| M9 | Foot Line | YES |
| M10 | Tack Ring Type | Press Ring – SR20 |
| M11 | Tack angle | 88.5 |
| M12 | Jack Line | No |
| M13 | Mast Bend (Luff Round) | Std |
| M14 | Fractional Rig (Yes, No) | Yes |
| M15 | Mast - Keel or Deck Stepped? | Keel |
| M16 | Number of Reefs | 3  Reefs |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | Yes, with 2 Eyelets for each reefing |
| M18 | Foot Reefing Grommets (next to boom) | N/A |
| M19 | Reefing Ring Type | Webbed ring for the luff with inside diameter 30mm,  1st Reef on Starboard max height 1900mm,  2nd reef on Portside max hight 850mm  Leech to have press Ring |
| M20 | Luff Length (Max Hoist - P) | 13.25m  Max  (Net Finished size day of Delivery) |
| M21 | Foot Length (Max Foot - E) | 4.450m  Max  (Net Finished size day of Delivery) |
| M22 | Leech Length (straight line head to clew) | Sailmaker |
| M23 | Bimini to Clear (yes or no) | N/A |
| M24 | Foot Round | Sailmaker |
| M25 | Aspect Ratio | Sailmaker |
| M26 | Vessel Backstay Measurement | N/A |
| M27 | Luff Slides (Part Number) |  |
| M28 | Foot Slides (Part Number) | Loose Footed |
| M29 | Roach Type | 1.1 |
| M30 | Roach Factor | 110 |
| M31 | MGM | Sailmaker |
| M32 | MGU | Sailmaker |
| M33 | Batten Type (Partial or Full) | 4 Full |
| M34 | Include Battens | Yes |
| M35 | Install Nylon Batten Holders |  |
| M36 | Intermediate Sliders | Webbing for bushing |
| M37 | Cloth Weight | DCX-M |
| M38 | Cut Type | Tri Radial |
| M39 | Sail Area |  |
| M40 | Cunningham | No |
| M41 | Telltails | Yes |
| M42 | Triple Stitch | Yes |
| M43 | Sail Logo and Color(red, blue or black) | Yes   Comfortina 35 logo (blue) |
| M44 | Sail Logo Artwork | N/A |
| M45 | Sail Numbers and Color | Yes  GER 138 (blue) |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Blue) |
| M47 | Overhead Leech Line | No |
| M48 | Specialty Sail | No |
| M49 | Boom Cover | No |
| M50 | Lazy Bag | Yes   Oyster |