H1 Size of Headsail (110, 135, 150 etc.): 105%

H2 Luff Length, Max Hoist, B measurement:

CAN'T MEASURE YET. WILL HAVE TO CLIMB TO THE MAST. TODAY I CAN INFORM THE FURLING BRAND AND MODEL.

H6 Clew Type (Press ring or 0-Ring): O-RING

H10 Track 1 (Tack to Genoa Track Beginning): 4.45 MT

H11 Track 2 (Tack to Genoa Track Ending) 4.80 MT

Diagrama

Descripción generada automáticamente

H17 Color of Sun cover: WHITE

H18 Side of Sail for Sun cover (port or Stbd): STBD (PHOTO)



H19 Luff Tape Size (such as #6): YOUR STANDARD.

H20 Furler Manufacturer: FACNOR LS 130

Imagen que contiene exterior, nieve, bicicleta, hecho de madera

Descripción generada automáticamente

Un helicóptero volando en el cielo

Descripción generada automáticamente con confianza mediaImagen que contiene edificio, espejo, vista, tabla

Descripción generada automáticamente

H25 Telltail Window: YES. PLEASE INCLUDE IN PRICE.

H31 Draft Stripe Color (red, blue, or black): BLACK

H32 Clew Height off Deck sailmaker: 38.0 CM

H33 Tack Height off Deck: 38.0 CM.

H34 Luff tape starts ??? up from Tack.: YOUR STANDARD.