|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Mainsail -  | 5000516 Robert |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | **85mm** | [HELP](Screenshot_2021-05-18%20Tack%20Cut%20Up%20and%20Cut%20Back.png)  |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | **25mm** | [HELP](Screenshot_2021-05-18%20Tack%20Cut%20Up%20and%20Cut%20Back.png)  |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | **30mm** | [HELP](Screenshot_2021-05-18%20Clew%20X%20and%20Y%20jpg%20%28JPEG%20Image%2C%20662%20%C3%97%20453%20pixels%29.png)  |
| M4 | Clew type (slug, outhaul car or ring with strap) | **See my email** | [HELP](Screenshot_2021-05-18%20Clew%20X%20and%20Y%20jpg%20%28JPEG%20Image%2C%20662%20%C3%97%20453%20pixels%29.png)  |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html)  |
| M6 | Other Offsets |  | [HELP](Screenshot_2021-05-18%20Boom_offsets.png)  |
| M7 | Headboard | Yes | [HELP](Screenshot_2021-05-18%20Head_Board_Types%20jpg%20%28JPEG%20Image%2C%20711%20%C3%97%201446%20pixels%29%20%E2%80%94%20Scaled%20%2871%25%29.png)  |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | **Press ring** | [HELP](Screenshot_2021-05-18%20Tack_Ring_Type%20html.png)  |
| M11 | Tack angle | 88.5 see photos | [HELP](Screenshot_2021-05-18%20Tack_Angle%20html.png)  |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.info/orderimages/Jack_Line.jpg)  |
| M13 | Mast Bend (Luff Round) | Std**45-50mm see photos** | [photo 4](photo%204.bmp) |
| M14 | Fractional Rig (Yes, No) | No | [HELP](Screenshot_2021-05-18%20Fractional%20Rig%20jpg%20%28JPEG%20Image%2C%20538%20%C3%97%20602%20pixels%29.png)  |
| M15 | Mast - Keel or Deck Stepped? | **Stepped** |  |
| M16 | Number of Reefs | 2  Reefs | [HELP](Screenshot_2021-05-18%20Reefs.png)  |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | yes | [HELP](Screenshot_2021-05-18%20Intermediate%20Reefing%20Tie%20Downs.png)  |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](Screenshot_2021-05-18%20Intermediate%20Reefing%20Tie%20Downs.png)  |
| M19 | Reefing Ring Type | **???** | [HELP](Screenshot_2021-05-18%20Reefing%20Ring%20Types.png)  |
| M20 | Luff Length (Max Hoist - P) | **10.52m? Max hoist height 10750mm**(Net Finished size day of Delivery) | [HELP](Screenshot_2021-05-18%20Mainsail%20Luff%20Measurement.png)  |
| M21 | Foot Length (Max Foot - E) | **3.80m?** Max**black band to mast aft face is3670mm** | [HELP](Screenshot_2021-05-18%20Mainsail%20foot%20Measurement.png)  |
| M22  | Leech Length (straight line head to clew) | Sailmaker | [HELP](Screenshot_2021-05-18%20Mainsail%20Leech%20Measurement%20Check.png)  |
| M23 | Bimini to Clear (yes or no) | YES | [HELP](Screenshot_2021-05-18%20Mainsail%20Bimini%20Check.png) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](Screenshot_2021-05-18%20Aspect%20Ratio.png) |
| M26 | Vessel Backstay Measurement | **4710** | [HELP](Screenshot_2021-05-18%20BoomArt2%20jpg%20%28JPEG%20Image%2C%20868%20%C3%97%20520%20pixels%29.png)  |
| M27 | Luff Slides (Part Number) | **See photos** | [HELP](Screenshot_2021-05-18%20sailslides3.png)  |
| M28 | Foot Slides (Part Number) | **Loose**  | [HELP](Screenshot_2021-05-18%20sailslides3.png)  |
| M29 | Roach Type | Cruise | [HELP](Screenshot_2021-05-18%20roach%20jpg%20%28JPEG%20Image%2C%20347%20%C3%97%20341%20pixels%29.png)  |
| M30 | Roach Factor | 1.1 | [HELP](Screenshot_2021-05-18%20Roach-Factor.png)  |
| M31 | MGM | Sailmaker | [HELP](Screenshot_2021-05-18%20Design%20MGM%20and%20MGU.png)  |
| M32 | MGU | Sailmaker | [HELP](Screenshot_2021-05-18%20Design%20MGM%20and%20MGU.png)  |
| M33 | Batten Type (Partial or Full) | 4 Partial | [HELP](Screenshot_2021-05-18%20Full%20Batten%20Options.png)  |
| M34 | Include Battens | YES |  |
| M35 | Install Nylon Batten Holders | N/A | [HELP](Screenshot_2021-05-18%20Fareastsails%20Full%20Batten%20Holder%20Options.png)  |
| M36 | Intermediate Sliders | YES | [HELP](Screenshot_2021-05-18%20Intermediate%20Sliders.png)  |
| M37 | Cloth Weight | 6oz Contender Radian |  |
| M38 | Cut Type | Tri Radial |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | No | [HELP](Screenshot_2021-05-18%20cunningham%20jpg%20%28JPEG%20Image%2C%20620%20%C3%97%201070%20pixels%29%20%E2%80%94%20Scaled%20%2896%25%29.png)  |
| M41 | Telltails | Yes | [HELP](Screenshot_2021-05-18%20Telltails.png)  |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](Screenshot_2021-05-18%20snlogos.png)  |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | No | [HELP](Screenshot_2021-05-18%20snlogos.png)  |
| M46 | Draft Stripe and Color(red, blue or black) | Yes Blue | [HELP](http://www.fareastsails.info/Draft%20Stripe.html)  |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](Screenshot_2021-05-18%20Lazy_Bag.png) |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Headsail - | 5000516 Robert |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | Luff Leech and Foot | [HELP](Screenshot_2021-05-18%20gen123%20jpg%20%28JPEG%20Image%2C%20399%20%C3%97%20413%20pixels%29.png)  |
| H2 | Luff Length, Max Hoist, B measurement | 10.78mwebbing loop tip to webbing loop tip (Max)**max furling** **11050**mgm = 1.95mmgl = 3.04mMgu =0.94mjgt = 0.48mjh = 0.07 | [HELP](Screenshot_2021-05-18%20Furler%20Luff%20Measurement.png)  |
| H3 | Leech Length | sailmaker | [HELP](Screenshot_2021-05-18%20Leech%20Length%20jpg%20%28JPEG%20Image%2C%20650%20%C3%97%20826%20pixels%29.png)  |
| H4 | Foot Length | sailmaker | [HELP](Screenshot_2021-05-18%20Foot%20Length%20jpg%20%28JPEG%20Image%2C%20662%20%C3%97%20776%20pixels%29.png)  |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | **O ring** | [HELP](Screenshot_2021-05-18%20genoa%20clew%20types%20jpg%20%28JPEG%20Image%2C%20558%20%C3%97%20783%20pixels%29.png)  |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | **4060** | [HELP](Genoa%20Track.pdf)  |
| H11 | Track 2 (Tack to Genoa Track Ending) | **5050** | [HELP](Genoa%20Track.pdf)  |
| H12 | Vessel "I" Measurement | **10550** | [HELP](Screenshot_2021-05-18%20Vessel%20I%20measurement.png)  |
| H13 | Vessel "J" Measurement | **3400** | [HELP](Screenshot_2021-05-18%20LP%2BI%2BJ.png)  |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | 4.16m | [HELP](Screenshot_2021-05-18%20LP%2BI%2BJ.png)  |
| H17 | Color of Suncover | **silver** | [HELP](Screenshot_2021-05-18%20Weather_Max_Colors.png)  |
| H18 | Side of Sail for Suncover (port or Stbd) | **Stbd** |  |
| H19 | Luff Tape Size (such as #6) | 5mm | [HELP](Screenshot_2021-05-18%20Furler_Luff_Tape.png)  |
| H20 | Furler Manufacturer | **Furlex 200s** |  |
| H21 | Foam Luff | Yes | [HELP](Screenshot_2021-05-18%20Foam_Luff.png)  |
| H22 | Cut Type | Tri Radial |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html)  |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 6oz Contender Radian |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg)  |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (**Black**) | [HELP](Screenshot_2021-05-18%20Draft%20Stripe.png)  |
| H32 | Clew Height off Deck | Sailmaker **850** | [HELP](Screenshot_2021-05-18%20clewheight%20jpg%20%28JPEG%20Image%2C%20681%20%C3%97%201323%20pixels%29%20%E2%80%94%20Scaled%20%2877%25%29.png)  |
| H33 | Tack Height off Deck | **500** | [HELP](Screenshot_2021-05-18%20clewheight%20jpg%20%28JPEG%20Image%2C%20681%20%C3%97%201323%20pixels%29%20%E2%80%94%20Scaled%20%2877%25%29.png)  |
| H34 | Luff tape starts **???**up from Tack | **950 from loop** | [HELP](Screenshot_2021-05-18%20Luff%20tape%20start%20jpg%20%28JPEG%20Image%2C%20600%20%C3%97%20800%20pixels%29.png) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |