|  |  |  |
| --- | --- | --- |
|  | - Mainsail - Bavaria 35 cruiser | 5000520 Sven |
| M0 | Sail Layout | Not Yet Posted |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | N/A |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | N/A |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | N/A |
| M4 | Clew type (slug, outhaul car or ring with strap) | Clew Block – Yes |
| M5 | Sunbrella clew cover for Furling Mains | Yes – Color : Royal Blue |
| M6 | Other Offsets | Luff tape start 10 cm up from tack.    Luff tape end 30 cm. |
| M7 | Headboard | Webbing Loops |
| M8 | Leech Line | yes |
| M9 | Foot Line | No |
| M10 | Tack Ring Type | Webbing Loops |
| M11 | Tack angle | Furling Mainsail – sailmakaer |
| M12 | Jack Line | No |
| M13 | Mast Bend (Luff Round) | Std |
| M14 | Fractional Rig (Yes, No) | No |
| M15 | Mast - Keel or Deck Stepped? | N/A |
| M16 | Number of Reefs | N/A Reefs |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | N/A |
| M18 | Foot Reefing Grommets (next to boom) | N/A |
| M19 | Reefing Ring Type | N/A |
| M20 | Luff Length (Max Hoist - P) | 11.90m  Max Webbing Loop to Webbing Loops  (11.78m Net Finished size day of Delivery) |
| M21 | Foot Length (Max Foot - E) | 4.10 m  Max  3.05 m  Max (Net Finished size day of Delivery) |
| M22 | Leech Length (straight line head to clew) | Sailmaker |
| M23 | Bimini to Clear (yes or no) |  |
| M24 | Foot Round | Sailmaker |
| M25 | Aspect Ratio | Sailmaker |
| M26 | Vessel Backstay Measurement | N/A |
| M27 | Luff Slides (Part Number) | Luff Tape Size 5 mm |
| M28 | Foot Slides (Part Number) | Loose Footed |
| M29 | Roach Type | Sailmaker |
| M30 | Roach Factor | Sailmaker |
| M31 | MGM | Sailmaker |
| M32 | MGU | Sailmaker |
| M33 | Batten Type (Partial or Full) | N/A |
| M34 | Include Battens | N/A |
| M35 | Install Nylon Batten Holders | N/A |
| M36 | Intermediate Sliders | N/A |
| M37 | Cloth Weight | 8.3oz Challenge Premium High Modulus Dacron - Cross Cut |
| M38 | Cut Type | Cross |
| M39 | Sail Area | Sailmaker |
| M40 | Cunningham | No |
| M41 | Telltails | Yes |
| M42 | Triple Stitch | Yes |
| M43 | Sail Logo and Color(red, blue or black) | No |
| M44 | Sail Logo Artwork | N/A |
| M45 | Sail Numbers and Color | No |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Blue) |
| M47 | Overhead Leech Line | No |
| M48 | Specialty Sail | No |
| M49 | Boom Cover | No |
| M50 | Lazy Bag | No |

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - Bavaria 35 cruiser | 5000520 Sven |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 115% | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 12.00m webbing loop tip to webbing loop tip (Max)  11.70m (Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg) |
| H4 | Foot Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg) |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 4.15 m | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | 6.10 m | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H12 | Vessel "I" Measurement | 12.10 m | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| H13 | Vessel "J" Measurement | 3.30 m | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | N/A |  |
| H15 | Reef | N/A |  |
| H16 | LP | N/A | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | Royal Blue | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | Starboard |  |
| H19 | Luff Tape Size (such as #6) | 5mm | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | Selden |  |
| H21 | Foam Luff | No | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 8.3oz Challenge Premium High Modulus Dacron - Cross Cut |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (Blue) | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html) |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | 0.45 m | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts ???up from Tack | 1.0 m | [HELP](http://www.fareastsails.infp/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |