|  |  |  |
| --- | --- | --- |
|  |  - Headsail - | 6000127 Kjell |
| H0 | Sail Layout | Not Yet Posted |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 14019,000 DPI |
| H2 | Luff Length, Max Hoist, B measurement | 20.08m webbing loop tip to webbing loop tip (Max)(Sailamker Net Finished size day of delivery) |
| H3 | Leech Length | sailmaker |
| H4 | Foot Length | sailmaker |
| H5 | Tack and Head Fittings | Webbing Loops |
| H6 | Clew Type (Press ring or 0-Ring) | Press Ring |
| H7 | Leech Line | Yes |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |
| H9 | Foot Line | Yes |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 5,567 m |
| H11 | Track 2 (Tack to Genoa Track Ending) | 9.157 m |
| H12 | Vessel "I" Measurement | 19.60 m from end of profile to deck20.03 m from mast termination to deck |
| H13 | Vessel "J" Measurement | 5.36 m |
| H14 | Calculated Forestay Length | Sailmaker |
| H15 | Reef | N/A |
| H16 | LP | Sailmkaer |
| H17 | Color of Suncover | N/A |
| H18 | Side of Sail for Suncover (port or Stbd) | N/A |
| H19 | Luff Tape Size (such as #6) | 5 mm Profurl finished size |
| H20 | Furler Manufacturer | Profurl |
| H21 | Foam Luff | N/A |
| H22 | Cut Type | Membrane |
| H23 | Sail Area | Sailmaker |
| H24 | Telltails | Yes |
| H25 | Telltail Window | No |
| H26 | Triple Stitch | YES |
| H27 | Logo | No |
| H28 | Cloth Weight | 4D Carbon Membrane with DP Lite Skin - Both sidesDPI: 19,000 |
| H29 | Sail Numbers and Color (red, blue or black) | RED |
| H30 | Sheeting Stripe (red, blue, black) | No |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (RED) |
| H32 | Clew Height off Deck | sailmaker |
| H33 | Tack Height off Deck | 0 cm (Shackle 10cm below deck) |
| H34 | Luff tape starts 50cm up from Tack | 50 cm |
| H35 | Specialty Sail | No |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  |