|  |  |  |  |
| --- | --- | --- | --- |
|  | - Mainsail - |  |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 98 mm | [HELP](http://www.fareastsails.info/orderimages/Tack%252520Cut%252520Up%252520and%252520Cut%252520Back.html) |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 10 mm | [HELP](http://www.fareastsails.info/orderimages/Tack%252520Cut%252520Up%252520and%252520Cut%252520Back.html) |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/Clew%252520X%252520and%252520Y.jpg) |
| M4 | Clew type (slug, outhaul car or ring with strap) | Slug,B012 | [HELP](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html) |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| M6 | Other Offsets | Harken battcar A system, 22 mm track, see attached photo | [HELP](http://www.fareastsails.info/orderimages/Boom_offsets.html) |
| M7 | Headboard | Yes, has to be compatible with Harken 22 mm CB headboard car assembly | [HELP](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg) |
| M8 | Leech Line | yes, led through top of Sail and down to Luff for adjustment (adjustment at each Reef point) |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | Webbed tack ring | [HELP](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html) |
| M11 | Tack angle | 88.5 | [HELP](http://www.fareastsails.info/orderimages/Tack_Angle.html) |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.info/orderimages/Jack_Line.jpg) |
| M13 | Mast Bend (Luff Round) | See photo | [HELP](http://www.fareastsails.info/orderimages/mastbend.jpg) |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.info/orderimages/Fractional%252520Rig.jpg) |
| M15 | Mast - Keel or Deck Stepped? | Deck |  |
| M16 | Number of Reefs | 3 deep Reefs, at third Reef the sail should be "storm sail" size | [HELP](http://www.fareastsails.info/orderimages/Reefs.html) |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | Yes | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M19 | Reefing Ring Type | Floppy Reefing rings | [HELP](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html) |
| M20 | Luff Length (Max Hoist - P) | 14.59 m  Max (measured to black band on mast) | [HELP](http://www.fareastsails.info/orderimages/Mainsail%252520Luff%252520Measurement.html) |
| M21 | Foot Length (Max Foot - E) | 4.82 m  Max (measured to black band on boom) | [HELP](http://www.fareastsails.info/orderimages/Mainsail_Foot_Measurement.html) |
| M22 | Leech Length (straight line head to clew) | Sailmaker (15.60 is the max) | [HELP](http://www.fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html) |
| M23 | Bimini to Clear (yes or no) | Yes/maybe. There is a hard dodger but it is not very tall. Boom parallel to the waterline is OK. Max leech measurement provided above for safety. Check also mast bend / backstay photos. | [HELP](http://www.fareastsails.info/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Aspect%252520Ratio.html) |
| M26 | Vessel Backstay Measurement | 6670. See also attached photo. | [HELP](http://www.fareastsails.info/orderimages/BoomArt2.jpg) |
| M27 | Luff Slides (Part Number) | Harken battcar system A, 22 mm track.  W144010 Holders | [HEyLP](http://www.fareastsails.info/orderimages/sailslides3.html) |
| M28 | Foot Slides (Part Number) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html) |
| M29 | Roach Type | 1.1 | [HELP](http://www.fareastsails.info/orderimages/roach.jpg) |
| M30 | Roach Factor | Cruise | [HELP](http://www.fareastsails.info/orderimages/Roach-Factor.html) |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%252520MGM%252520and%252520MGU.html) |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%252520MGM%252520and%252520MGU.html) |
| M33 | Batten Type (Partial or Full) | Full batten | [HELP](http://www.fareastsails.info/orderimages/Full%252520Batten%252520Options.html) |
| M34 | Include Battens | Yes |  |
| M35 | Install Nylon Batten Holders | W144010 Holders Harken Battcar A system (22 mm track) | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com%252520Full%252520Batten%252520Holder%252520Options.html) |
| M36 | Intermediate Sliders | N/A | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html) |
| M37 | Cloth Weight | 9.88 |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | Yes | [HELP](http://www.fareastsails.info/orderimages/cunningham.jpg) |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (red) | [HELP](http://www.fareastsails.info/Draft%252520Stripe.html) |
| M47 | Overhead Leech Line | Yes |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%252520Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.info/orderimages/Lazy_Bag.html) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - |  |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 110% | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 15830 mm webbing loop tip to webbing loop tip (Max)  (Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%252520Length.jpg) |
| H4 | Foot Length | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%252520Length.jpg) |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | O-ring | [HELP](http://www.fareastsails.info/orderimages/genoa%252520clew%252520types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 7100 mm | [HELP](http://www.fareastsails.info/orderimages/Genoa%252520Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | 9000 mm | [HELP](http://www.fareastsails.info/orderimages/Genoa%252520Track.pdf) |
| H12 | Vessel "I" Measurement | 16450 mm | [HELP](http://www.fareastsails.info/orderimages/Vessel%252520I%252520measurement.html) |
| H13 | Vessel "J" Measurement | 4990 mm | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sail | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | Scarlet | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | Sb |  |
| H19 | Luff Tape Size (such as #6) | HL7 #7 | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | Selden 404s |  |
| H21 | Foam Luff | Yes | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 9.88 fastnet |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%252520Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (red) | [HELP](http://www.fareastsails.info/orderimages/Draft%252520Stripe.html) |
| H32 | Clew Height off Deck | sailmaker / high-cut genoa, around 1.6-1.8 m off the deck. | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | 540 mm | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts 540mm up from Tack | 540 mm | [HELP](http://www.fareastsails.info/orderimages/Luff%252520tape%252520start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%252520Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | staysail |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 100% approx | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 10340 mm webbing loop tip to webbing loop tip (Max)  (Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%252520Length.jpg) |
| H4 | Foot Length | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%252520Length.jpg) |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | O-ring | [HELP](http://www.fareastsails.info/orderimages/genoa%252520clew%252520types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | Track will be installed at the same time with the sail, suggested measurement: 3100 mm, track 183 cm apart at the beginning | [HELP](http://www.fareastsails.info/orderimages/Genoa%252520Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | Suggested measurement: 4000 mm, track 220cm apart at the end | [HELP](http://www.fareastsails.info/orderimages/Genoa%252520Track.pdf) |
| H12 | Vessel "I" Measurement | 10760 mm | [HELP](http://www.fareastsails.info/orderimages/Vessel%252520I%252520measurement.html) |
| H13 | Vessel "J" Measurement | 3265 mm | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sail | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | Scarlet | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | Sb |  |
| H19 | Luff Tape Size (such as #6) | HL7 #7 | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | Selden 304s |  |
| H21 | Foam Luff | Yes | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 9.88 fastnet |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%252520Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (red) | [HELP](http://www.fareastsails.info/orderimages/Draft%252520Stripe.html) |
| H32 | Clew Height off Deck | sailmaker (should be closer to deck) | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | 285 mm | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts 540mm up from Tack | 540 mm | [HELP](http://www.fareastsails.info/orderimages/Luff%252520tape%252520start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%252520Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |