|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Mainsail -  | 6000807 Matteo |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 80mm | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 50mm | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/Clew%20X%20and%20Y.jpg)  |
| M4 | Clew type (slug, outhaul car or ring with strap) | Press Ring | [HELP](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html)  |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html)  |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.info/orderimages/Boom_offsets.html)  |
| M7 | Headboard | Yes | [HELP](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg)  |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | Press Ring | [HELP](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html)  |
| M11 | Tack angle | Lagoon 400 | [HELP](http://www.fareastsails.info/orderimages/Tack_Angle.html)  |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.info/orderimages/Jack_Line.jpg)  |
| M13 | Mast Bend (Luff Round) | Std | [HELP](http://www.fareastsails.info/orderimages/mastbend.jpg)  |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.info/orderimages/Fractional%20Rig.jpg)  |
| M15 | Mast - Keel or Deck Stepped? | N/A |  |
| M16 | Number of Reefs | 3  Reefs | [HELP](http://www.fareastsails.info/orderimages/Reefs.html)  |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | Yes | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M19 | Reefing Ring Type | Press Ring Luff and Leech | [HELP](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html)  |
| M20 | Luff Length (Max Hoist - P) | 15.400m  Max(15.246m Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.info/orderimages/Mainsail%20Luff%20Measurement.html)  |
| M21 | Foot Length (Max Foot - E) | 5.200m  Max(5.14m Net Finished size day of Delivery)  | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Foot_Measurement.html)  |
| M22  | Leech Length (straight line head to clew) | Sailmaker | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html)  |
| M23 | Bimini to Clear (yes or no) |  | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | N/A | [HELP](http://www.fareastsails.info/orderimages/BoomArt2.jpg)  |
| M27 | Luff Slides (Part Number) | ??? | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html)  |
| M28 | Foot Slides (Part Number) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html)  |
| M29 | Roach Type | CAT | [HELP](http://www.fareastsails.info/orderimages/roach.jpg)  |
| M30 | Roach Factor | 135% | [HELP](http://www.fareastsails.info/orderimages/Roach-Factor.html)  |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  |
| M33 | Batten Type (Partial or Full) | 5 Full | [HELP](http://www.fareastsails.info/orderimages/Full%20Batten%20Options.html)  |
| M34 | Include Battens | Checking |  |
| M35 | Install Nylon Batten Holders | Checking  | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html)  |
| M36 | Intermediate Sliders | Checking  | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html)  |
| M37 | Cloth Weight | 9.88 fastnet |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | No | [HELP](http://www.fareastsails.info/orderimages/cunningham.jpg)  |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html)  |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Black) | [HELP](http://www.fareastsails.info/Draft%20Stripe.html)  |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.info/orderimages/Lazy_Bag.html) |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Headsail - | Lagoon 400 |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 95% | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg)  |
| H2 | Luff Length, Max Hoist, B measurement | 14.93mwebbing loop tip to webbing loop tip (Max)(14.78m Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html)  |
| H3 | Leech Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg)  |
| H4 | Foot Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg)  |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg)  |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 5450mm | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf)  |
| H11 | Track 2 (Tack to Genoa Track Ending) | 6300mm | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf)  |
| H11B | Track Height Above the Deck | 1110mm |  |
| H12 | Vessel "I" Measurement | 15.36m | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html)  |
| H13 | Vessel "J" Measurement | 4.10m | [HELP](http://www.fareastsails.info/orderimages/LP%2BI%2BJ.html)  |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sailmaker  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg)  |
| H17 | Color of Suncover | TAUPE  | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html)  |
| H18 | Side of Sail for Suncover (port or Stbd) | STBD |  |
| H19 | Luff Tape Size (such as #6) | 5mm Finished | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html)  |
| H20 | Furler Manufacturer | FacnorLS200 |  |
| H21 | Foam Luff | Yes | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html)  |
| H22 | Cut Type | Cross |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html)  |
| H25 | Telltail Window | No |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight |  |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg)  |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (color ?) | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html)  |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg)  |
| H33 | Tack Height off Deck | 480mm | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg)  |
| H34 | Luff tape starts 500mmup from Tack | 500mm | [HELP](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |