Catalina 30 Tall Rig

Luff = 36’ 9’’

Foot = 12.00

Leach = 38.78

|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Mainsail -  | 6001214 Philippe |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 1.875in | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 1.25in | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/Clew%20X%20and%20Y.jpg)  |
| M4 | Clew type (slug, outhaul car or ring with strap) | O-Ring w/slug no. B102  | [HELP](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html)  |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html)  |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.info/orderimages/Boom_offsets.html)  |
| M7 | Headboard | Yes | [HELP](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg)  |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | Webbed Tack O-Ring  | [HELP](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html)  |
| M11 | Tack angle | 88.5 – See luff leech and foot | [HELP](http://www.fareastsails.info/orderimages/Tack_Angle.html)  |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.info/orderimages/Jack_Line.jpg)  |
| M13 | Mast Bend (Luff Round) | Std | [HELP](http://www.fareastsails.info/orderimages/mastbend.jpg)  |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.info/orderimages/Fractional%20Rig.jpg)  |
| M15 | Mast - Keel or Deck Stepped? | Deck stepped |  |
| M16 | Number of Reefs | 2  Reefs | [HELP](http://www.fareastsails.info/orderimages/Reefs.html)  |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | YES | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M19 | Reefing Ring Type | Floppy reefing ring3.5in between rings | [HELP](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html)  |
| M20 | Luff Length (Max Hoist - P) | 36’ 9’’ MaxNet = 36.382ft | [HELP](http://www.Fareastsails.info/orderimages/Mainsail%20Luff%20Measurement.html)  |
| M21 | Foot Length (Max Foot - E) | 12’ MaxNet = 11.88ft | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Foot_Measurement.html)  |
| M22  | Leech Length (straight line head to clew) | 38.78 MaxNet Sailmaker | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html)  |
| M23 | Bimini to Clear (yes or no) | yes | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | 187in | [HELP](http://www.fareastsails.info/orderimages/BoomArt2.jpg)  |
| M27 | Luff Slides (Part Number) | A009 | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html)  |
| M28 | Foot Slides (Part Number) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html)  |
| M29 | Roach Type | Cruise | [HELP](http://www.fareastsails.info/orderimages/roach.jpg)  |
| M30 | Roach Factor | 1.1 | [HELP](http://www.fareastsails.info/orderimages/Roach-Factor.html)  |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  |
| M33 | Batten Type (Partial or Full) | Full Batten | [HELP](http://www.fareastsails.info/orderimages/Full%20Batten%20Options.html)  |
| M34 | Include Battens | N/A |  |
| M35 | Install Nylon Batten Holders | YES | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html)  |
| M36 | Intermediate Sliders | YES2 | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html)  |
| M37 | Cloth Weight | 6.68 Fastnet |  |
| M38 | Cut Type | Cross |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | No | [HELP](http://www.fareastsails.info/orderimages/cunningham.jpg)  |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html)  |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| M46 | Draft Stripe and Color(red, blue or black) | Yes / blue | [HELP](http://www.fareastsails.info/Draft%20Stripe.html)  |
| M47 | Overhead Leech Line | No |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.info/orderimages/Lazy_Bag.html) |

Footnote 1

Actual slug on my main is a A type (but my measurements are 72mm long, 12 mm diameter so that’s why I put B102)

But Catalina specs is 3 ¼ long, ½ diameter, so more like A033.

Not sure what to choose here.



Footnote 2 – This is the right sail slide I need with correct measurement. I guess it’s your A009.



Philippe Dubois

1804, rue Grou

Longueuil, Quebec

Canada

J4N 1H5