
1 = N/A Do not need

2 = **Check tomorrow**

3 = **40 mm**

4 = 85mm

5 = **12 mm from aft side of profile (profile height is 15 mm)**

6 = 85mm

7 = **49** **mm from aft side of profile** **(profile height is 15 mm)**

8 = 10mm **M10**

9 = **195 mm**

10 = **62** **mm from aft side of profile (profile height is 15 mm)**

11 = 12 mm

12 = **MAX** 14mm

|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Square Top Mainsail - Lavezzi 40 Catamaran | 6000122 Björn |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | **45mm** | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | **35** aft of mast trackBottom of tack need chafing protection  | [HELP](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/Clew%20X%20and%20Y.jpg)  |
| M4 | Clew type (slug, outhaul car or ring with strap) | **MAXI O RING diameter min 50 mm+ Velcro band length 1,8 meter** | [HELP](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html)  |
| M5 | Sunbrella clew cover for Furling Mains | na | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html)  |
| M6 | Other Offsets |  | [HELP](http://www.fareastsails.info/orderimages/Boom_offsets.html)  |
| M7 | Headboard | Maxi Ring with pin 12mm **in headboard car**Fat head about 1,6 metersmax thickness 14mm of headboard | [HELP](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg)  |
| M8 | Leech Line | Yes with clamcleat |  |
| M9 | Foot Line | No |  |
| M10 | Tack Ring Type | ~~Press Ring~~ **Stainless O-ring** | [HELP](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html)  |
| M11 | Tack angle | 84 degrees – Leech **check relative distance from head to clew** | [HELP](http://www.fareastsails.info/orderimages/Tack_Angle.html)  |
| M12 | Jack Line | No | [HELP](http://www.fareastsails.info/orderimages/Jack_Line.jpg)  |
| M13 | Mast Bend (Luff Round) | Mast has a permanent bend of about 60mm (at upper spreader)  Mast is leaning backwards quite a lot. 53 mm per meter at deck level. (More higher up because of permanent mast bend.)  | [HELP](http://www.fareastsails.info/orderimages/mastbend.jpg)  |
| M14 | Fractional Rig (Yes, No) | No | [HELP](http://www.fareastsails.info/orderimages/Fractional%20Rig.jpg)  |
| M15 | Mast - Keel or Deck Stepped? | N/A |  |
| M16 | Number of Reefs | 3  ReefsReef 1 front 2150 rear 2120 from sail corner Reef 2 front 1950 rear 1970 from reef 1 Reef 3 front 1945 rear 1950 from reef 2Note: Locations for the reefs on the existing sail measured along front- and rear edges of the sail: Measuring point on the reef is inner side at the bottom of the stainless ring. | [HELP](http://www.fareastsails.info/orderimages/Reefs.html)  |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | Yes 4 **pcs** only the 1st reef**Plus:**4 **pcs** Extra eyelets locations: Nr 1: 350 mm from the front edge of the sail 750 mm from the bottom of the sail Nr 2: 1940 mm from the front edge of the sail 710 mm from the bottom of the sail Nr 3: 2020 mm from the rear edge of the sail 610 mm from the bottom of the sail Nr 4: 480 mm from the rear edge of the sail 360 mm from the bottom of the sail | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M18 | Foot Reefing Grommets (next to boom) | N/A | [HELP](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  |
| M19 | Reefing Ring Type | 3 ReefsLuff and Leech: O ring for blocks: reef 1 and 2 – StarboardReef 3: Port Side | [HELP](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html)  |
| M20 | Luff Length (Max Hoist - P) | 13.940  Max **Note: Goose neck 300 mm higher on mast than sail drawing.**(13.80m Net Finished size day of Delivery) | [HELP](http://www.Fareastsails.info/orderimages/Mainsail%20Luff%20Measurement.html)  |
| M21 | Foot Length (Max Foot - E) | 5.700m  Max(5.64m Net Finished size day of Delivery)  | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Foot_Measurement.html)  |
| M22  | Leech Length (straight line head to clew) | Sailmaker – See tack angle info**Compare with measurement from top to clew. Difficult to measure angle.** | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html)  |
| M23 | Bimini to Clear (yes or no) | N/A **End of boom never below XXX mm over deck KOLLA** | [HELP](http://www.Fareastsails.info/orderimages/Mainsail_Bimini_Check.html) |
| M24 | Foot Round | Sailmaker |  |
| M25 | Aspect Ratio | Sailmaker **Suggestion?** | [HELP](http://www.fareastsails.info/orderimages/Aspect%20Ratio.html) |
| M26 | Vessel Backstay Measurement | No Backstay - Catamaran | [HELP](http://www.fareastsails.info/orderimages/BoomArt2.jpg)  |
| M27 | Luff Slides (Part Number) | Car System - Z-spars **mast** about 250x150 | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html)  |
| M28 | Foot Slides (Part Number) | Loose Footed | [HELP](http://www.fareastsails.info/orderimages/sailslides3.html)  |
| M29 | Roach Type | See batten Lengths | [HELP](http://www.fareastsails.info/orderimages/roach.jpg)  |
| M30 | Roach Factor | See batten Lengths | [HELP](http://www.fareastsails.info/orderimages/Roach-Factor.html)  |
| M31 | MGM | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  |
| M32 | MGU | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  |
| M33 | Batten Type (Partial or Full) | Note: Measured from end to end of the battensBottom to top1: 4995mm 2: 4385 mm3: 3650mm 4: 2842mm5: 2078mm **(Front end only in batten pocket not full length, no batten car or holder)**6: 1918mm7: Fat head batten: 1772 mm **front end close to batten nr 6, no separate batten car but batten holder se photo)** | [HELP](http://www.fareastsails.info/orderimages/Full%20Batten%20Options.html)  |
| M34 | Include Battens | N/A |  |
| M35 | Install Nylon Batten Holders | YesLuff: **6 pcs** **Rutgersson** W1590 - 10mm Leech: heavy Duty Velcro Pocket**Velcro??? Batten installed from front end and adjusted in batten holder (except batten nr 5).****Strong anti chafe material both sides of all batten pockets** | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html)  |
| M36 | Intermediate Sliders | Yes – Webbing1. Batten car 1 2. Intermediate car with webbing to sail 3. Batten car 2 4. Intermediate car with webbing to sail 5. Batten car 3 6. Intermediate car with webbing to sail 7. Batten car 4 8. Intermediate car with webbing to sail **Intermediate cars: Webbing width 25mm. Vertical opening for 12 mm bushing. Pls test all!**9. Batten car 5 and fathead batten. Special bolt M10, existing. **– Client will install** **??? Yes, no difference for sailmaker compared to other batten cars M10 inside thread.**10. Top traveller. Bolt through head board.  | [HELP](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html)  |
| M37 | Cloth Weight | 9.65 FIBERCON® PRO HYBRID POWERED WITH DYNEEMA - TRI RADIAL |  |
| M38 | Cut Type | TRI RADIAL |  |
| M39 | Sail Area | Sailmaker |  |
| M40 | Cunningham | ~~No~~ **YES in spec!** | [HELP](http://www.fareastsails.info/orderimages/cunningham.jpg)  |
| M41 | Telltails | Yes | [HELP](http://www.fareastsails.info/orderimages/telltails.html)  |
| M42 | Triple Stitch | Yes |  |
| M43 | Sail Logo and Color(red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| M44 | Sail Logo Artwork | N/A |  |
| M45 | Sail Numbers and Color |  SWE 10978 – (Blue) **2 lines Stitched to sail.** | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| M46 | Draft Stripe and Color(red, blue or black) | Yes (Blue) | [HELP](http://www.fareastsails.info/Draft%20Stripe.html)  |
| M47 | Overhead Leech Line | Yes |  |
| M48 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| M49 | Boom Cover | No | [HELP](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M50 | Lazy Bag | No | [HELP](http://www.fareastsails.info/orderimages/Lazy_Bag.html) |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  - Headsail - | 6000122 Björn |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | See Luff Leech and Foot | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg)  |
| H2 | Luff Length, Max Hoist, B measurement | 13.060m webbing loop tip to webbing loop tip (Max)(12.92m Net Finished size day of delivery) | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html)  |
| H3 | Leech Length | 11.615m | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg)  |
| H4 | Foot Length | 5.890m | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg)  |
| H5 | Tack and Head Fittings | Webbing LoopsTack needs Chafing Protection. Starts at 220 mm from tack, length 950 mm. |  |
| H6 | Clew Type (Press ring or 0-Ring) | Press Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg)  |
| H7 | Leech Line | Yes. **No lose lines after clam cleat. Must be velcro pocket or similar. Risk of hooking up something on mast othervise.** |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs  |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 6.140m **1105 from centerline boat** | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf)  |
| H11 | Track 2 (Tack to Genoa Track Ending) | 6.590m **1340 from centerline boat** | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf)  |

|  |  |  |  |
| --- | --- | --- | --- |
| H12 | Vessel "I" Measurement | **Doublecheck tomorrow****See sail drawing XXX from deck (maststep) to halyard sheave****YYY from deck (maststep) to forstay fitting in mast** | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html)  |
| H13 | Vessel "J" Measurement | **3.740mm front side mast to bolt forstay**. **Deck level is not well defined. Could also be 3770 measured to “deck level” 😊 See photo.** | [HELP](http://www.fareastsails.info/orderimages/LP%2BI%2BJ.html)  |
| H14 | Calculated Forestay Length | **See sail drawing Check tomorrow** |  |
| H15 | Reef | Compensator (double check) **YES** |  |
| H16 | LP | Sailmaker **(Old sail 5310 pls.check)**  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg)  |
| H17 | Color of Suncover | Ocean Blue - Sunbrella | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html)  |
| H18 | Side of Sail for Suncover (port or Stbd) | Port Side |  |
| H19 | Luff Tape Size (such as #6) | 5mm | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html)  |
| H20 | Furler Manufacturer | Profurl C430 |  |
| H21 | Foam Luff | Yes **Please advise foam or rope. Ropes fixed individually to sail? Bad experience of ropes making a very thick bump! Foam gives wrinkles…** | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html)  |
| H22 | Cut Type | Tri Radial |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes, **also when reefed** | [HELP](http://www.fareastsails.info/orderimages/telltails.html)  |
| H25 | Anti chafe | Anti chafe for the spreader**s**:Mid point from clew 3680 mm and 7900mm from top.Height 500 mm in aft end and 150 mm in front end. Length 580 mm.**AND** **XXX for upper spreader. We will check location when it’s less windy. Hopefully tomorrow!****Both sides.** |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | 9.65 FIBERCON® PRO HYBRID POWERED WITH DYNEEMA - Tri Radial |  |
| H29 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html)  |
| H30 | Sheeting Stripe (red, blue, black) | No | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg)  |
| H31 | Draft Stripe Color  (red, blue or black) | Yes (Blue) | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html)  |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg)  |
| H33 | Tack Height off Deck | 470mm **From center of forstay bolt. 530 from deck.** | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg)  |
| H34 | Luff tape starts 830 mm up from Tack | 830 mm **XX Double Check tomorrow.** | [HELP](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |