Spécial notes :

At the top of the sail, the measurement between top of the bord and the sheave is 300 mm but, the sail could only be hoisted about 200mm more due to the eye splice and shackle length.

-Measurements are all taken while the sails are fully stretched to their maximum using conditions.

-The head sail, as no clearance at the top, IT IS AT ITS MAXIMUM HOIST!