|  |  |  |  |
| --- | --- | --- | --- |
|  | -  - | **3000215 Mario** |  |
| S0 | Sail Layout | Not Yet Posted |  |
| S1 | Size of Headsail (110, 135, 150 etc.)" | A3  130m2 |  |
| S2 | Luff Length, Max Hoist, B measurement | Sailmaker | [HELP](http://www.fareastsails.com/Gennaker%20Furler%20Luff%20Measurement.html) |
| S3 | Leech Length | sailmaker |  |
| S4 | Foot Length | sailmaker |  |
| S5 | Tack and Head Fittings | O-Rings |  |
| S6 | Vessel "I" Measurement | 16.7m | [HELP](http://www.fareastsails.com/orderimages/Vessel%20I%20measurement.html) |
| S7 | Vessel "J" Measurement | 4.70m | [HELP](http://www.fareastsails.com/orderimages/LP+I+J.html) |
| S8 | Calculated Forestay Length | N/A |  |
| S9 | Masthead or Fractional Spinnaker ? | **???** |  |
| S10 | Tack up for Code 0's | N/A |  |
| S11 | Correct Size for A/Spin or S/Spin | 130m2 |  |
| S12 | LP | N/A | [HELP](http://www.fareastsails.com/orderimages/LP.jpg) |
| S13 | Cut Type | Full Radial |  |
| S14 | U/V Cover | No |  |
| S15 | Luff Type | Free |  |
| S16 | Furler Name | None |  |
| S17 | Sail Area | 130m3 |  |
| S18 | Cloth Weight | 150 Maxlite |  |
| S19 | Sail Colors | To be provided | [HELP](http://www.fareastsails.com/orderimages/Spinnaker_Colors.html) |
| S20 | Sail Numbers and Color (red, blue or black) | No | [HELP](http://www.fareastsails.com/orderimages/snlogos.html) |
| S21 | Sail Logo | No |  |
| S22 | Sail Sock (White is std Color) | **???** |  |
| S23 | Sail Sock Length | YES |  |
| S24 | Wire Size | N/A |  |
| S25 | Sail Sock Color | **???** | [HELP](http://www.fareastsails.com/orderimages/Fareastsails_Spinnaker_Sock_Colors.html) |
| S26 | Specialty Sail |  | [HELP](http://www.fareastsails.com/orderimages/Specialty%20Sails.html) |
| S27 | Score |  | [HELP](http://www.fareastsails.com/orderimages/Score.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.com/orderimages/LP.jpg) |