|  |  |  |  |
| --- | --- | --- | --- |
|  | - Mainsail - | 4000907 Claudio |  |
| M0 | Sail Layout | Not Yet Posted |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | 5cm | [HEL](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  [P](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | 8cm | [HEL](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html)  [P](http://www.fareastsails.info/orderimages/Tack%20Cut%20Up%20and%20Cut%20Back.html) |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | 5cm | [HEL](http://www.fareastsails.info/orderimages/Clew%20X%20and%20Y.jpg)  [P](http://www.fareastsails.info/orderimages/Clew%20X%20and%20Y.jpg) |
| M4 | Clew type (slug, outhaul car or ring with strap) | slug | [HEL](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html)  [P](http://www.fareastsails.info/orderimages/Clew_Types_Fareastsails.html) |
| M5 | Sunbrella clew cover for Furling Mains | na | [HEL](http://www.fareastsails.info/orderimages/weathermax_colors.html)  [P](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| M6 | Other Offsets |  | [HEL](http://www.fareastsails.info/orderimages/Boom_offsets.html)  [P](http://www.fareastsails.info/orderimages/Boom_offsets.html) |
| M7 | Headboard | Yes | [HEL](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg)  [P](http://www.fareastsails.info/orderimages/Head_Board_Types.jpg) |
| M8 | Leech Line | yes |  |
| M9 | Foot Line | No |  |
| M1 0 | Tack Ring Type | tack press ring | [HEL](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html)  [P](http://www.fareastsails.info/orderimages/Tack_Ring_Type.html) |
| M1 1 | Tack angle | 88.5 | [HEL](http://www.fareastsails.info/orderimages/Tack_Angle.html)  [P](http://www.fareastsails.info/orderimages/Tack_Angle.html) |
| M1 2 | Jack Line | No | [HEL](http://www.fareastsails.info/orderimages/Jack_Line.jpg)  [P](http://www.fareastsails.info/orderimages/Jack_Line.jpg) |
| M1 3 | Mast Bend (Luff Round) | Std | [HEL](http://www.fareastsails.info/orderimages/mastbend.jpg)  [P](http://www.fareastsails.info/orderimages/mastbend.jpg) |
| M1 4 | Fractional Rig (Yes, No) | yes | [HEL](http://www.fareastsails.info/orderimages/Fractional%20Rig.jpg)  [P](http://www.fareastsails.info/orderimages/Fractional%20Rig.jpg) |
| M1 5 | Mast - Keel or Deck Stepped? | deck |  |
| M1 6 | Number of Reefs | 2 Reefs | [HEL](http://www.fareastsails.info/orderimages/Reefs.html)  [P](http://www.fareastsails.info/orderimages/Reefs.html) |

|  |  |  |  |
| --- | --- | --- | --- |
| M1 7 | Intermediate Reefing Diamond Eyes (Yes or No) | yes | [HEL](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  [P](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M1 8 | Foot Reefing Grommets (next to boom) | yes | [HEL](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html)  [P](http://www.fareastsails.info/orderimages/Intermediate_Reefing_Tie_Downs.html) |
| M1 9 | Reefing Ring Type | floppy standard | [HEL](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html)  [P](http://www.fareastsails.info/orderimages/Reefing_Ring_Types.html) |
| M2 0 | Luff Length (Max Hoist - P) | 9.40 mt  Max  (Net Finished size day of Delivery) | [HEL](http://www.fareastsails.info/orderimages/Mainsail%20Luff%20Measurement.html)  [P](http://www.fareastsails.info/orderimages/Mainsail%20Luff%20Measurement.html) |
| M2 1 | Foot Length (Max Foot - E) | 3.2mt  Max  (Net Finished size day of Delivery) | [HEL](http://www.fareastsails.info/orderimages/Mainsail_Foot_Measurement.html)  [P](http://www.fareastsails.info/orderimages/Mainsail_Foot_Measurement.html) |
| M2 2 | Leech Length (straight line head to clew) | Sailmaker | [HEL](http://www.fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html)  [P](http://www.fareastsails.info/orderimages/Mainsail_Leech_Measurement_Check.html) |
| M2 3 | Bimini to Clear (yes or no) |  | [HEL](http://www.fareastsails.info/orderimages/Mainsail_Bimini_Check.html)  [P](http://www.fareastsails.info/orderimages/Mainsail_Bimini_Check.html) |
| M2 4 | Foot Round | Sailmaker |  |
| M2 5 | Aspect Ratio | Sailmaker | [HEL](http://www.fareastsails.info/orderimages/Aspect%20Ratio.html)  [P](http://www.fareastsails.info/orderimages/Aspect%20Ratio.html) |
| M2 6 | Vessel Backstay Measurement | 3.8mt | [HEL](http://www.fareastsails.info/orderimages/BoomArt2.jpg)  [P](http://www.fareastsails.info/orderimages/BoomArt2.jpg) |
| M2 7 | Luff Slides (Part Number) | A007 | [HEL](http://www.fareastsails.info/orderimages/sailslides3.html)  [P](http://www.fareastsails.info/orderimages/sailslides3.html) |
| M2 8 | Foot Slides (Part Number) | A017S | [HEL](http://www.fareastsails.info/orderimages/sailslides3.html)  [P](http://www.fareastsails.info/orderimages/sailslides3.html) |
| M2 9 | Roach Type | Cruise | [HEL](http://www.fareastsails.info/orderimages/roach.jpg)  [P](http://www.fareastsails.info/orderimages/roach.jpg) |
| M3 0 | Roach Factor | 1.1 | [HEL](http://www.fareastsails.info/orderimages/Roach-Factor.html)  [P](http://www.fareastsails.info/orderimages/Roach-Factor.html) |
| M3 1 | MGM | Sailmaker | [HEL](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  [P](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html) |
| M3 2 | MGU | Sailmaker | [HEL](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html)  [P](http://www.fareastsails.info/orderimages/Design%20MGM%20and%20MGU.html) |

|  |  |  |  |
| --- | --- | --- | --- |
| M3 3 | Batten Type (Partial or Full) | 4 Full | [HEL](http://www.fareastsails.info/orderimages/Full%20Batten%20Options.html)  [P](http://www.fareastsails.info/orderimages/Full%20Batten%20Options.html) |
| M3 4 | Include Battens | NO |  |
| M3 5 | Install Nylon Batten Holders | YES | [HEL](http://www.fareastsails.info/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html)  [P](http://www.fareastsails.info/orderimages/Fareastsails.com%20Full%20Batten%20Holder%20Options.html) |
| M3 6 | Intermediate Sliders | YES  2 | [HEL](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html)  [P](http://www.fareastsails.info/orderimages/Fareastsails.com_Intermediate_Full_Batten_Sliders.html) |
| M3 7 | Cloth Weight | 6.63 |  |
| M3 8 | Cut Type | Cross |  |
| M3 9 | Sail Area | Sailmaker |  |
| M4 0 | Cunningham | No | [HEL](http://www.fareastsails.info/orderimages/cunningham.jpg)  [P](http://www.fareastsails.info/orderimages/cunningham.jpg) |
| M4 1 | Telltails | Yes | [HEL](http://www.fareastsails.info/orderimages/telltails.html)  [P](http://www.fareastsails.info/orderimages/telltails.html) |
| M4 2 | Triple Stitch | Yes |  |
| M4 3 | Sail Logo and Color(red, blue or black) | No | [HEL](http://www.fareastsails.info/orderimages/snlogos.html)  [P](http://www.fareastsails.info/orderimages/snlogos.html) |
| M4 4 | Sail Logo Artwork | N/A |  |
| M4 5 | Sail Numbers and Color | No | [HEL](http://www.fareastsails.info/orderimages/snlogos.html)  [P](http://www.fareastsails.info/orderimages/snlogos.html) |
| M4 6 | Draft Stripe and Color(red, blue or black) | Yes (Color?) | [HEL](http://www.fareastsails.info/Draft%20Stripe.html)  [P](http://www.fareastsails.info/Draft%20Stripe.html) |
| M4 7 | Overhead Leech Line | No |  |
| M4 8 | Specialty Sail | No | [HEL](http://www.fareastsails.info/orderimages/Specialty%20Sails.html)  [P](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| M4 9 | Boom Cover | No | [HEL](http://www.fareastsails.info/orderimages/Boom_Cover.html)  [P](http://www.fareastsails.info/orderimages/Boom_Cover.html) |
| M5 0 | Lazy Bag | No | [HEL](http://www.fareastsails.info/orderimages/Lazy_Bag.html)  [P](http://www.fareastsails.info/orderimages/Lazy_Bag.html) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | 4000907 Claudio |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 110 | [HEL](http://www.fareastsails.info/orderimages/gen123.jpg)  [P](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | webbing loop tip to webbing loop tip (Max)  (Net Finished size day of delivery) | [HEL](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html)  [P](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | sailmaker | [HEL](http://www.fareastsails.info/orderimages/Leech%20Length.jpg)  [P](http://www.fareastsails.info/orderimages/Leech%20Length.jpg) |
| H4 | Foot Length | sailmaker | [HEL](http://www.fareastsails.info/orderimages/Foot%20Length.jpg)  [P](http://www.fareastsails.info/orderimages/Foot%20Length.jpg) |
| H5 | Tack and Head Fittings | Webbing Loops |  |
| H6 | Clew Type (Press ring or 0-Ring) | o ring | [HEL](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg)  [P](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H1 0 | Track 1 (Tack to Genoa Track Beginning) | 3.25mt | [HEL](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf)  [P](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H1 1 | Track 2 (Tack to Genoa Track Ending) | 5.6mt | [HEL](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf)  [P](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H1 2 | Vessel "I" Measurement | 9.91m | [HEL](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html)  [P](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| H1 3 | Vessel "J" Measurement | 3.14m | [HEL](http://www.fareastsails.info/orderimages/LP%2BI%2BJ.html)  [P](http://www.fareastsails.info/orderimages/LP%2BI%2BJ.html) |
| H1 4 | Calculated Forestay Length | Sailmaker |  |
| H1 5 | Reef | N/A |  |
| H1 6 | LP | Sailmaker | [HEL](http://www.fareastsails.info/orderimages/LP.jpg)  [P](http://www.fareastsails.info/orderimages/LP.jpg) |
| H1 7 | Color of Suncover | silver cwm382 | [HEL](http://www.fareastsails.info/orderimages/weathermax_colors.html)  [P](http://www.fareastsails.info/orderimages/weathermax_colors.html) |

|  |  |  |  |
| --- | --- | --- | --- |
| H1 8 | Side of Sail for Suncover (port or Stbd) | port |  |
| H1 9 | Luff Tape Size (such as #6) | #8 | [HEL](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html)  [P](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H2 0 | Furler Manufacturer | unknown |  |
| H2 1 | Foam Luff | YES | [HEL](http://www.fareastsails.info/orderimages/Foam_Luff.html)  [P](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H2 2 | Cut Type | Cross |  |
| H2 3 | Sail Area | Sailmaker |  |
| H2 4 | Telltails | Yes | [HEL](http://www.fareastsails.info/orderimages/telltails.html)  [P](http://www.fareastsails.info/orderimages/telltails.html) |
| H2 5 | Telltail Window | No |  |
| H2 6 | Triple Stitch | YES |  |
| H2 7 | Logo | No | [HEL](http://www.fareastsails.info/orderimages/snlogos.html)  [P](http://www.fareastsails.info/orderimages/snlogos.html) |
| H2 8 | Cloth Weight | 6.63 |  |
| H2 9 | Sail Numbers and Color (red, blue or black) | No | [HEL](http://www.fareastsails.info/orderimages/snlogos.html)  [P](http://www.fareastsails.info/orderimages/snlogos.html) |
| H3 0 | Sheeting Stripe (red, blue, black) | No | [HEL](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg)  [P](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg) |
| H3 1 | Draft Stripe Color (red, blue or black) | Yes (blue) | [HEL](http://www.fareastsails.info/orderimages/Draft%20Stripe.html)  [P](http://www.fareastsails.info/orderimages/Draft%20Stripe.html) |
| H3 2 | Clew Height off Deck | sailmaker | [HEL](http://www.fareastsails.info/orderimages/clewheight.jpg)  [P](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H3 3 | Tack Height off Deck | 65cm | [HEL](http://www.fareastsails.info/orderimages/clewheight.jpg)  [P](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H3 4 | Luff tape starts ???  up from Tack | 40cm | [HEL](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg)  [P](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H3 5 | Specialty Sail | No | [HEL](http://www.fareastsails.info/orderimages/Specialty%20Sails.html)  [P](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are |  | [HEL](http://www.fareastsails.info/orderimages/LP.jpg)  [P](http://www.fareastsails.info/orderimages/LP.jpg) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | based on accurate vessel I and J Measurements |  |  |