|  |  |  |
| --- | --- | --- |
|  |  - Mainsail - | 6000718 Val |
| M0 | Sail Layout |  |
| M1 | Tack Cut Back (Aft face of Mast to center of tack Pin - A) | N/A |
| M2 | Tack Cut Up (Top of Boom to Center of tack Pin - B) | N/A |
| M3 | Clew Cut Up (Top of Boom to Center of Tack Pin - X) | N/A |
| M4 | Clew type (slug, outhaul car or ring with strap) | Press Ring |
| M5 | Sunbrella clew cover for Furling Mains | na |
| M6 | Other Offsets |  |
| M7 | Headboard | Yes |
| M8 | Leech Line | Yes |
| M9 | Foot Line | No |
| M10 | Tack Ring Type | Press Ring |
| M11 | Tack angle | Luff Leech and Foot |
| M12 | Jack Line | No |
| M13 | Mast Bend (Luff Round) | Std |
| M14 | Fractional Rig (Yes, No) | No |
| M15 | Mast - Keel or Deck Stepped? | Keel |
| M16 | Number of Reefs | 3  Reefs |
| M17 | Intermediate Reefing Diamond Eyes (Yes or No) | YES |
| M18 | Foot Reefing Grommets (next to boom) | NO |
| M19 | Reefing Ring Type | Grommet through sail |
| M20 | Luff Length (Max Hoist - P) | **40' 0"  Max12.307575 meters NET** |
| M21 | Foot Length (Max Foot - E) | **21'1"  Max( 20.76 feet Net Finished size day of Delivery)** |
| M22 | Leech Length (straight line head to clew) | **42'2" Max41.53 ft NET** |
| M23 | Bimini to Clear (yes or no) | N/A |
| M24 | Foot Round | Sailmaker |
| M25 | Aspect Ratio | Sailmer |
| M26 | Vessel Backstay Measurement | N/A |
| M27 | Luff Slides (Part Number) | **???** |
| M28 | Foot Slides (Part Number) | **Loose footed6 Gromments on foot for Nonsuch LinesGrommets Spaced2'6, 5'10, 8'5, 11'9, 15'2, 18'1.Sailmaker, please note mast is forward part of the vessel.** |
| M29 | Roach Type | See design |
| M30 | Roach Factor | See design |
| M31 | MGM | Sailmaker |
| M32 | MGU | Sailmaker |
| M33 | Batten Type (Partial or Full) | Partial |
| M34 | Include Battens | yes |
| M35 | Install Nylon Batten Holders | N/A |
| M36 | Intermediate Sliders | N/A |
| M37 | Cloth Weight | 7.3 HM |
| M38 | Cut Type | Cross |
| M39 | Sail Area | Sailmaker |
| M40 | Cunningham | No |
| M41 | Telltails | Yes |
| M42 | Triple Stitch | Yes |
| M43 | Sail Logo and Color(red, blue or black) | N/A |
| M44 | Sail Logo Artwork | N/A |
| M45 | Sail Numbers and Color | N/A |
| M46 | Draft Stripe and Color(red, blue or black) | No |
| M47 | Overhead Leech Line | No |
| M48 | Specialty Sail | No |
| M49 | Boom Cover | No |
| M50 | Lazy Bag | No |