*Headsail Number 1*

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | 7000110 James |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 155 | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 8.6M Max | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg) |
| H4 | Foot Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg) |
| H5 | Tack and Head Fittings (Press ring or 0-Ring) | O-Ring |  |
| H6 | Clew Type (Press ring or 0-Ring) | O-Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 3.47M | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | 4.89M | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H12 | Vessel "I" Measurement | 8.72m | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| H13 | Vessel "J" Measurement | 2.80m | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | Sailmaker | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | N/A | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | N/A |  |
| H19 | Luff Tape Size (such as #6) or Piston Hanks | Piston Hanks | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | N/A |  |
| H21 | Foam Luff | N/A | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Tri Radial |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes  Can I Get 2 Top Leech Telltales As well | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | Yes |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | DP: PX05 Black - Tri Radial |  |
| H29 | Sail Numbers and Color (red, blue or black) | RED IRL 81641 | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | Black | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | RED | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html) |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | 30mm | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts N/A up from Tack | N/A | [HELP](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |

*Headsail Number 2*

|  |  |  |  |
| --- | --- | --- | --- |
|  | - Headsail - | 7000110 James |  |
| H0 | Sail Layout | Not Yet Posted |  |
| H1 | Size of Headsail (110, 135, 150 etc.)" | 105% Horizontal Battens | [HELP](http://www.fareastsails.info/orderimages/gen123.jpg) |
| H2 | Luff Length, Max Hoist, B measurement | 8.6M Max | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Measurement.html) |
| H3 | Leech Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Leech%20Length.jpg) |
| H4 | Foot Length | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Foot%20Length.jpg) |
| H5 | Tack and Head Fittings (Press ring or 0-Ring) | O-Ring |  |
| H6 | Clew Type (Press ring or 0-Ring) | O-Ring | [HELP](http://www.fareastsails.info/orderimages/genoa%20clew%20types.jpg) |
| H7 | Leech Line | Yes |  |
| H8 | Reefs for Hank on Sail (specify Qty of tiedowns) | No Manual Reefs |  |
| H9 | Foot Line | Yes |  |
| H10 | Track 1 (Tack to Genoa Track Beginning) | 3.47M | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H11 | Track 2 (Tack to Genoa Track Ending) | 4.89M | [HELP](http://www.fareastsails.info/orderimages/Genoa%20Track.pdf) |
| H12 | Vessel "I" Measurement | 8.72m | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| H13 | Vessel "J" Measurement | 2.80m | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| H14 | Calculated Forestay Length | Sailmaker |  |
| H15 | Reef | N/A |  |
| H16 | LP | N/A | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| H17 | Color of Suncover | N/A | [HELP](http://www.fareastsails.info/orderimages/weathermax_colors.html) |
| H18 | Side of Sail for Suncover (port or Stbd) | N/A |  |
| H19 | Luff Tape Size (such as #6)or Piston Hanks | Piston Hanks | [HELP](http://www.fareastsails.info/orderimages/Furler_Luff_Tape.html) |
| H20 | Furler Manufacturer | N/A |  |
| H21 | Foam Luff | N/A | [HELP](http://www.fareastsails.info/orderimages/Foam_Luff.html) |
| H22 | Cut Type | Tri Radial |  |
| H23 | Sail Area | Sailmaker |  |
| H24 | Telltails | Yes  Can I Get 2 Top Leech Telltales Aswell | [HELP](http://www.fareastsails.info/orderimages/telltails.html) |
| H25 | Telltail Window | Yes |  |
| H26 | Triple Stitch | YES |  |
| H27 | Logo | No | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H28 | Cloth Weight | DP: PX10 Black - Tri Radial |  |
| H29 | Sail Numbers and Color (red, blue or black) | RED IRL 81641 | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| H30 | Sheeting Stripe (red, blue, black) | Black | [HELP](http://www.fareastsails.info/orderimages/Sheeting%20Stripe.jpg) |
| H31 | Draft Stripe Color  (red, blue or black) | RED | [HELP](http://www.fareastsails.info/orderimages/Draft%20Stripe.html) |
| H32 | Clew Height off Deck | sailmaker | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H33 | Tack Height off Deck | 30mm | [HELP](http://www.fareastsails.info/orderimages/clewheight.jpg) |
| H34 | Luff tape starts N/A up from Tack | N/A | [HELP](http://www.fareastsails.info/orderimages/Luff%20tape%20start.jpg) |
| H35 | Specialty Sail | No | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |

*Symmetrical Spinnaker*

|  |  |  |  |
| --- | --- | --- | --- |
|  | -  - | 7000110 James |  |
| S0 | Sail Layout | Not Yet Posted |  |
| S1 | Size of Headsail (110, 135, 150 etc.)" | Symmetrical Spinnaker |  |
| S2 | Luff Length, Max Hoist, B measurement | sailmaker | [HELP](http://www.fareastsails.info/orderimages/Gennaker%20Furler%20Luff%20Measurement.html) |
| S3 | Leech Length | sailmaker |  |
| S4 | Foot Length | sailmaker |  |
| S5 | Tack and Head Fittings | O-Rings |  |
| S6 | Vessel "ISP" Measurement | 9.2m | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| S7 | Vessel "TPS" Measurement | 3.00m | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |
| S8 | Calculated Forestay Length | Sailmaker |  |
| S9 | Masthead or Fractional Spinnaker ? | Fractional Spinnaker |  |
| S10 | Tack up for Code 0's | N/A |  |
| S11 | Correct Size for A/Spin or S/Spin | N/A |  |
| S12 | LP | N/A | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |
| S13 | Cut Type | Full Radial |  |
| S14 | U/V Cover | N/A |  |
| S15 | Luff Type | Free |  |
| S16 | Furler Name | None |  |
| S17 | Sail Area | ~41.75m2 |  |
| S18 | Cloth Weight | Contender Superlite 50 |  |
| S19 | Sail Colors | Pink / Black | [HELP](http://www.fareastsails.info/orderimages/Spinnaker_Colors.html) |
| S20 | Sail Numbers and Color (red, blue or black) | RED IRL 81641 | [HELP](http://www.fareastsails.info/orderimages/snlogos.html) |
| S21 | Sail Logo | No |  |
| S22 | Sail Sock (White is std Color) | No |  |
| S23 | Sail Sock Length | N/A |  |
| S24 | Wire Size | N/A |  |
| S25 | Sail Sock Color |  | [HELP](http://www.fareastsails.info/orderimages/Fareastsails_Spinnaker_Sock_Colors.html) |
| S26 | Specialty Sail |  | [HELP](http://www.fareastsails.info/orderimages/Specialty%20Sails.html) |
| S27 | Score |  | [HELP](http://www.fareastsails.info/orderimages/Score.html) |
|  | Customer Note: All details we can check as sailmakers are based on accurate vessel I and J Measurements |  | [HELP](http://www.fareastsails.info/orderimages/LP.jpg) |

|  |  |  |  |
| --- | --- | --- | --- |
| S6 | Vessel "ISP" Measurement | 9.2M | [HELP](http://www.fareastsails.info/orderimages/Vessel%20I%20measurement.html) |
| S7 | Vessel "TPS" Measurement | 3M | [HELP](http://www.fareastsails.info/orderimages/LP+I+J.html) |